EV Charge Station V2 firmware change log
[bookmark: _heading=h.gjdgxs]Product
The EV Charge Station V2 has three-phase and single-phase capabilities. It delivers maximum 22kW AC in three-phase mode or 7.3kW in single-phase mode.
It incorporates a 4.3-inch LCD touch screen for monitoring and control and a fully programmable RGB Light Ring around the charging port, to quickly determine the device state.
[bookmark: _heading=h.30j0zll]How to update?
This product can be updated in three different ways:
· Update remotely over the internet via our VRM Portal. It requires a GX device, such as a Color Control GX, Venus GX or Cerbo GX to be part of the installation.
· Update via the internal web interface. Open the internal web interface and go to Settings->FW Update. 
For an online update, open the ‘Online updates’ tab and click the ‘Press to check’ button. The device will check whether a new firmware version is available. If a new version is found, click ‘Press to update to’ to start the update. 
To update using a firmware file, open the ‘Offline updates’ tab. Click ‘Open’ and select the ‘*.evcsup’ firmware file. Then click ‘Update’ and wait until the update procedure is complete. 
The ‘*.evcsup’ firmware files can be downloaded from the Victron Professional website.
· Update via the VictronConnect app. Connect to your device using the VictronConnect app. If a new firmware version is available, the app will display a dedicated update notification. Follow the instructions in the app to perform the firmware update.

Documentation for VRM: Remote firmware update is here.
[bookmark: _heading=h.1fob9te]What firmware version do I currently have?
There are several ways to see the firmware version:
· Look at the System-overview page on the VRM Portal
· Look on the left-bottom corner of the EV Charging Station LCD
· Look on the left-bottom corner of the EV Charging Station web interface
[bookmark: _heading=h.3znysh7]How to configure?
EV Charge Station V2 can be fully configured via built-in web interface or VictronConnect app. Please check this video tutorial.
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v1.02 - 19 October 2026

New features:
· Extended the First-setup procedure for VictronConnect app to match the functionality available in the web interface

Improvements:
· System performance and stability improvements

v1.01 - 5 October 2026

First approved version for mass production



